Q3 Coffee Grinder User Manual
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[image: ]1 Preface
[bookmark: bookmark20]Please  read  this   manual  carefully   before  using  the  appliance,   because  the manual   contains    important    instructions   for   the   safety,   operation    and maintenance   of   the    appliance.    Please   keep    this    manual   properly.   The manufacturer reserves the right to make and change the product and manual.

When  opening  the   package,  please  check  carefully  to   make  sure  that  the appliance  does  not  show  any  signs  of  damage.   If  you  have  any  questions, please do not use the device and contact a qualified professional.

Packaging materials must be placed out of the reach of children, because such materials  may pose a  potential threat to children.  Please  keep this  packaging until the end of the warranty period.

Do  not throw  away  at will.  Please  dispose  of  the  packaging  materials  of  the product in accordance with relevant laws and regulations.
You decide not to use the device, please be sure to unplug the power plug to ensure the safety of the electrical appliance. For information on the disposal of electrical components, please consult a professional company.

This appliance is designed to grind coffee beans. To avoid danger, please do not use  this  appliance  for  other  purposes.  The  manufacturer  will   not  bear  any responsibility for any danger caused by improper use or incorrect use.

Do not use the coffee bean bin to store other products or weigh other foods.
This electrical appliance is only suitable for  professional  use  by  professionals, the user  must be an adult, and children are not allowed to use the electrical equipment.
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[bookmark: bookmark3][bookmark: bookmark21]2 Product Configurat ion [image: ]
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	Hopper cover     1 PC
	Bean Hopper     1PC
	Main body     1 PC

	Powder tray 1 PC
	Power Line     1PC
	User manual     1PC



Noise level
EEC countries:
The maximum noise level of our product is 78 dB(A). Test distance: 30cm away from the machine.
United States and Canada:
The noise level of electrical appliances is included in the US regulations 29 CFR
1910.95 ( ‘ Occupational Health and Environment Control- Occupational noise exposure ’ ),  and it can  be exposed for 8  hours a day (the  noise exposure is limited to the operation of the equipment).
The same new electrical appliance has been determined to be the above noise level.
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	Model
	Q3
	Hopper capacity
	750g

	Voltage
	220V-240V
	Frequency
	50/60HZ

	Power
	420W
	Rotate Speed
	1800 rpm

	Blades Material
	Stainless steel
	Size of blades
	64mm flat burr

	Machine Size
	165x255x475mm
	Meas.
	390x225x510mm

	G.W.
	10.05KGS
	N.W.
	8.55KGS
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[bookmark: bookmark23][bookmark: bookmark5][image: ]4 Placement&Wir ing

The appliance must be installed by professional and technical personnel.
Incorrect installation may cause personal injury or product damage, for which the manufacturer will not bear any responsibility.
Clean  the  device  carefully  after  installation,  please  follow  the  cleaning  and maintenance instructions.
	[image: ]①The electrical appliance must be placed in a stable position, and the recommended distance from the ground is 80-100cm.
② Before plugging in the appliance, make sure that the socket voltage  matches the frequency and the data on the appliance technical label. Ensure that the rating of the system meets the electrical consumption rate—as indicated on the technical data label, and that the socket used is protected against overcurrent.
③The  socket  must  be  equipped  with  an  effective  grounding device to ensure that the grounding system is effective.  If you fail to  comply with the  regulations,  the  manufacturer will  not bear any responsibility.
④ Do  not  use  extension cables,  multi-socket  plug  adapters or temporary connection devices.
⑤In  EEC  member  states, current  regulations  require that the external equipotential terminal on the electrical  base  must  be connected   to   the    equipotential   node    to   achieve    correct installation.
⑥The  motor  rotates clockwise. The  reverse  motor  cannot  be used, and the operation of this machine must be performed by professional technicians.
⑦This equipment  is only suitable for indoor  use.  Do  not  use this equipment outdoors.
⑧ Do   not   install   the   device   near   the   water   dispenser   or accidentally spill water on the device.
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[bookmark: bookmark7]5.1 Control panel set up
[image: ]Manual
Grinding time

Plus
Minor

5.4 Grind time set up

Long press the plus, after hearing the sound of bee, press minor
to set up, press the set up button to confirm.

5.5 Grinding mode set up

Long press set up button to hear the sound of bee, press the decrease, C1 shows manual mode, C2 shows auto mode, then press the manual button to confirm
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[bookmark: bookmark14]6.1 Maintenance
- The user must regularly check the working condition of the power cord and plug.
-   When  the   power   cord   or   plug   is   damaged,   please   ask   professional technicians to replace it to prevent danger.
- For CE certified electrical appliances, special tools are required to open the bottom plate to maintain the wires.
- We recommend using only original spare parts.
- In order to ensure the long-term effectiveness of electrical appliances, it is necessary to ask professional and technical personnel to carry out regular maintenance, including detailed inspection of the use status of parts that may be worn out.
- The condition of the grinding blade must be checked regularly. Please keep the grinding blade in good condition to ensure high-quality grinding, so as to improve work efficiency and avoid overheating.

[bookmark: bookmark15]6.2 Cleaning Preparation
- Before cleaning, please pull out the power plug to disconnect the electrical power.
- Do not use water spray to clean the appliance.
- Do not install electrical appliances in rooms where water sprays are used for cleaning.
-  Appliances  can  only  be  cleaned   regularly  by  professional  and  technical personnel.
- Do not use corrosive products, as such products may tarnish shiny parts.
- Please contact professional and technical personnel for a thorough cleaning operation if necessary.
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[bookmark: bookmark16][bookmark: bookmark28]6.3 Hopper Cleaning
- Before cleaning, please pull out the power plug to disconnect the electrical power.
- Do not use water spray to clean the appliance.
- Do not install electrical appliances in  rooms where water sprays are used for cleaning.
-  Appliances  can  only  be  cleaned  regularly   by  professional  and  technical personnel.
- Do not use corrosive products, as such products may tarnish shiny parts.
- Please contact professional and technical personnel for a thorough cleaning operation if necessary.

[bookmark: bookmark17][bookmark: _GoBack]
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[bookmark: bookmark18]7 Precaut ions [image: ]
The use of this appliance must comply with the relevant laws and regulations for safe operation.
.   When   operating   electrical   appliances,   pay   attention   to   the   movable mechanical   parts  of  the  grinding   blade  and  the  coffee  powder  outlet. Disconnect the power supply before removing the stocker from the grinding system. Without unplugging the power plug of the appliance, do not remove the impurities in the grinding system or the accumulator.
. Be careful when cleaning, because even if the appliance is turned off, the grinding blade may continue to rotate for a short time.
.  The  coffee  bean   hopper  must  be  fixed  to  the  grinding   system  of  the appliance with the supplied screws. The screws must not be inserted into the threaded  holes  on  the  upper  grinding  blade  clamp  and  the  holes  on  the hopper tube. The user is not allowed to remove any screws or parts on the appliance without authorization.
.  If  the  electrical  appliance  fails  to  work  normally  or  malfunctions,  please contact professional and technical personnel, and do not repair it yourself.
.  Before  performing  any  electrical  operations  (including  cleaning  and/or  maintenance), please unplug the power plug to disconnect the power source. Using the main switch to turn off the appliance cannot ensure safe operation  of the appliance. Do not modify electrical appliances.
.  When  the  electrical  appliance  is  left  unattended  (for  example,  at  night, during breaks, mid-week closures or holidays), the main switch must be used to turn off the electrical power.
. The internal or external parts of the appliance must not come into contact with any liquid.
.  The  hopper  can  only  be  used  to  store  coffee  beans,  do  not  put  coffee powder into the hopper.
. Do not pull the power cord to pull out the power plug of the appliance.
. Do not touch the appliance with wet hands or feet.
. Do not go barefoot when using electrical appliances.
If you fail to comply with the above regulations, the manufacturer will not be liable for any personal injury or property damage.
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	Date
	
	Product name&Model
	

	Serial Number
	

	Username
	
	Phone/Mobile
	

	Address
	

	


Problem
	

	

Repair
result
	





Repair person:                                   Date:

	The warranty period of this machine is one year (calculated from the day it      leaves the factory). During the warranty period, if the fault is caused by the     quality of the product itself, please contact our customer service staff for free accessories or replacement services.

The range of accessories provided for compensation in the following cases:
1. Without warranty proof.
2. Failures caused by operating the machine not in accordance with the requirements of the manual.
3. Failure, scratches or damage caused by moving or falling.
4. Damage caused by inappropriate preservation, maintain or usage.
5. Easy damaged pieces and present accessories are not concerned.
6. Failure or damage caused by force majeure.
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